Init bus...
VCC: 3.3 V, VCCQ: 1.8 V
Bus: 1 bit (SDR 24MHz)
Access mode: sector mode
Power supply: dual-voltage (1.70-1.95V, 2.7-3.6V)
 Card/BGA: BGA (Discrete embedded) - High density MMC
 Manufacturer ID: 0x15 (Samsung)
 Product name: QE13MB (0x514531334d42), rev: 0x07, serial number: 0xE87DF229
 Manufacturing date: Aug 2016
CID: 15010051 4531334D 4207E87D F2298390
CSD: D0270132 0F5903FF F6DBFFEF 8E40400C
EXT_CSD revision: 1.8 (MMC v5.1) 
Partition info:
 Boot1: 4096 KiB
 Boot2: 4096 KiB
 RPMB: 4096 KiB
 User area: 14.56 GiB(15,634,268,160 bytes)
