
EMMC Manufacturer ID: 0090 , OEM ID: 014A
EMMC Date: 08/2015  Rev.0x3
EMMC NAME: HAG2e  , S/N: 4204895445
EMMC NAME (HEX): 48414732652000 
EMMC ROM1 (Main User Data)   Capacity: 15032 MB
EMMC ROM2 (Boot Partition 1) Capacity: 4096 kB
EMMC ROM3 (Boot Partition 2) Capacity: 4096 kB
EMMC RPMB (Replay Protected Memory Block) Capacity: 4096 kB
EMMC Permanent Write Protection: No
EMMC Temporary Write Protection: No
EMMC Password Locked: No
  Extended CSD rev 1.7 (MMC 5.0)
Boot configuration [PARTITION_CONFIG: 0x48] Boot from:ROM2 (Boot Partition 1)
Boot bus config [177]: 0x00 , width 1bit  , Partition config [179]: 0x48.
H/W reset function [RST_N_FUNCTION]: 0x01
High-capacity W protect group size [HC_WP_GRP_SIZE: 0x00000000]
Partitioning Support [PARTITIONING_SUPPORT]: 0x07
 Device support partitioning feature
 Device can have enhanced tech.
Partitioning Setting [PARTITION_SETTING_COMPLETED]: 0x00
---------------------------------------------
Backup saved: HAG2e _4204895445_20170322_2108.extcsd
Done.