Done.

Z3X EasyJtag Software ver. 2.0.0.0
Loading eMMC Addon Firmware... IO: 2800 mV
Box S/N: 0201001B9BA01510, ,FW Ver.: 01.52
CMD Pullup Level:2124 mV
CMD Active Level:2670 mV
eMMC Device Information
EMMC CID : 90014A4834473164048602A3B6C4418E
EMMC CSD : D02701320F5903FFFFFFFFE78A4040E2
EMMC Manufacturer ID: 0090 , OEM ID: 014A
EMMC Date: 04/2014 Rev.0x86
EMMC NAME: H4G1d , S/N: 44283588
EMMC NAME (HEX): 48344731642000 
EMMC ROM1 (Main User Data) Capacity: 3696 MB
EMMC ROM2 (Boot Partition 1) Capacity: 2048 kB
EMMC ROM3 (Boot Partition 2) Capacity: 2048 kB
EMMC RPMB (Replay Protected Memory Block) Capacity: 2048 kB
EMMC Permanent Write Protection: No
EMMC Temporary Write Protection: No
Extended CSD rev 1.5 (MMC 4.41)
Boot configuration [PARTITION_CONFIG: 0x38] Boot from:ROM1 (Main User Area)
Boot bus config [177]: 0x00 , width 1bit , Partition config [179]: 0x38.
Backup saved: H4G1d _ 44283588_20150505_1758.extcsd
Searching for partition tables...
Detected GPT over MBR...
Medium UUID: 98101B32-BBE2-4BF2-A06E-2BB33D000C20
Warning: Entries Count = 28
MMCBLK0P0 (SBL1) Range: [0X4400,0X84200] ,Len: 80000
MMCBLK0P1 (SDI) Range: [0X84400,0X8C200] ,Len: 8000
MMCBLK0P2 (DDR) Range: [0X400000,0X407E00] ,Len: 8000
MMCBLK0P3 (RPM) Range: [0X800000,0X87CE00] ,Len: 7D000
MMCBLK0P4 (TZ) Range: [0X87D000,0X8F9E00] ,Len: 7D000
MMCBLK0P5 (ABOOT) Range: [0X8FA000,0XE6FE00] ,Len: 576000
MMCBLK0P6 (PAD) Range: [0XE70000,0XF6FE00] ,Len: 100000
MMCBLK0P7 (OEMINFO) Range: [0XF70000,0X4F6FE00] ,Len: 4000000
MMCBLK0P8 (MODEMST1) Range: [0X4F70000,0X536FE00] ,Len: 400000
MMCBLK0P9 (MODEMST2) Range: [0X5370000,0X576FE00] ,Len: 400000
MMCBLK0P10 (MODEM) Range: [0X5800000,0XB7FFE00] ,Len: 6000000
MMCBLK0P11 (FSG) Range: [0XB800000,0XBBFFE00] ,Len: 400000
MMCBLK0P12 (FSC) Range: [0XBC00000,0XBC00200] ,Len: 400
MMCBLK0P13 (SSD) Range: [0XBC00400,0XBC02200] ,Len: 2000
MMCBLK0P14 (LOG) Range: [0XBC02400,0XDC02200] ,Len: 2000000
MMCBLK0P15 (BKBOOTUP) Range: [0XE000000,0X11FFFE00] ,Len: 4000000
MMCBLK0P16 (PERSIST) Range: [0X12000000,0X127FFE00] ,Len: 800000
MMCBLK0P17 (BOOT) Range: [0X12800000,0X133FFE00] ,Len: C00000
MMCBLK0P18 (RECOVERY) Range: [0X13400000,0X143FFE00] ,Len: 1000000
MMCBLK0P19 (CUST) Range: [0X14400000,0X243FFE00] ,Len: 10000000
MMCBLK0P20 (CACHE) Range: [0X24400000,0X303FFE00] ,Len: C000000
MMCBLK0P21 (MISC) Range: [0X30400000,0X307FFE00] ,Len: 400000
MMCBLK0P22 (SYSTEM) Range: [0X30800000,0X707FFE00] ,Len: 40000000
MMCBLK0P23 (USERDATA) Range: [0X70800000,0XB07FFE00] ,Len: 40000000
MMCBLK0P24 (GROW) Range: [0XB0800000,0XE6FFBC00] ,Len: 367FBE00
Done...Presets has been updated...